Exercise 7\_Reading an ASCII-encoded string

s214417 Lukas Schou

s214413 Christian Cederhorn

Code to control the RGB ratio, when three integers are put into the serial monitor divided by commas:

*e.g. 200,140,50*

Et billede, der indeholder tekst, skærmbillede, Font/skrifttype, dokument

Automatisk genereret beskrivelse

Questions

* 7a: What is a RGB value? Why does it use the interval 0-255?

An RGB value is the ratio between the three parameters RED, GREEN and BLUE. The interval 0-255 is used because the values are stored using 8 bits or 1 byte

* 7b: What does the function Serial.parseInt() do?

The function reads an integer from the serial monitor until it meets a non-digit.